


Fieldbus Configuration: Modbus RTU




Gateway Configuration: Generic Data Mode.



Subnetwork Configuration. RS485. Baudrate: 57600 (minimum speed of the sensor). 8-E-1




Node Configuration: Slave Addr. 1




Consume transaction.


In order to avoid the LED#5 on in red (transaction error/Time out or subnet stopped) I put the offline timeout time in 0. Is this ok??




Consume Data:



Produce Transaction:





Anybus Configuration switch, Status and connections

